Standby generator unit			
	
Unit power		kW	
Power factor cos φ			
Power that must be substituted immediately after power failure		kW	
Notes on consumers 
(heavy starting or special features; e.g. frequency converter, UPS, power supply unit)			
Frequency converter on standby power supply		VA	
UPS load on standby power supply		VA	
Rated voltage		V	
Rated frequency		Hz	
Power supply system			
	TN-S		TN-C-S			TN-C			
	TT		IT			TN-S (EMC-friendly)	
Design class			
	G1		G2			G3		G4	
			
Fuel			
	Gas			Gasoline	
	Diesel fuel			
Required operating time at rated power without refueling		h	
Type of cooling for combustion engine			Air cooling	
			Liquid cooling	
Operating mode			Time-limited operation	
			Emergency power unit	
			Peak load unit	
			Stand-alone	
			Parallel operation with the power	
			In parallel with other power generating units	
Expected annual operating hours		h	
Type of installation			Stationary	
			Transportable	
			Mobile	
Power generating unit			With long interruption time	
			Quick-starting standby generator unit	
			No-break standby generator unit	
Effects of weather			Indoor	
			Outdoor	
			Open air installation	
Ambient temperature		°C	
Installation altitude (above sea level)		m	
Air pollution			
	Sand/dust			Chemicals	
			
Noise limit (maximum level)		dB	
Emissions			
Exhaust gas emission limits			
Dimensions (width × depth × height)		m   x	m   x	m	
Weight		kg	

With the completed list you have gained an overview of the project.
Do you need detailed information e.g. about concept development or budget estimation?
With the data contained in the checklist, contact your responsible TIP contact person:	
Totally Integrated Power supports electrical designers in different planning stages with software tools, Revit files for Building Information Modeling (BIM), tender specification texts, planning and application manuals and professional consulting by our experienced technical specialists in many countries: www.siemens.com/tip-cs

Get in touch with us: www.siemens.com/tip-cs/contact