Busbar trunking systems			
Project name			
Owner/developer			
Planning engineer			
Rated operating voltage		V	
Rated current (dependent on degree of protection and lying method)		A	
Ambient temperature		°C	
Degree of protection		IP	
Supply system			
	TN-S		TN-C-S			TN-C			
	TT		IT			TN-S (EMC-friendly)	
Design-verified connection to the LVMD			Yes			
Conductor configuration			
	L1, L2, L3		N			2N			
	PE		        PE			PE = casing	
			
Maximum voltage drop 
(from supply to busbar to the final load feeder)			
Number of fire walls (wall bushings)			
Proportion of busbars with fire walls		(in m)	
Fastening/routing of busbar			
Busbar layout drawing (incl. lengths and loads)			

With the completed list you have gained an overview of the project.
Do you need detailed information e.g. about concept development or budget estimation?
With the data contained in the checklist, contact your responsible TIP contact person:	
Totally Integrated Power supports electrical designers in different planning stages with software tools, Revit files for Building Information Modeling (BIM), tender specification texts, planning and application manuals and professional consulting by our experienced technical specialists in many countries: www.siemens.com/tip-cs

Get in touch with us: www.siemens.com/tip-cs/contact