Activity Guide 2

**Safety:**

* Attach the wire samples for testing to a ruler so the ends cannot flick into your eyes

Equipment:

Micrometer screw gauge to measure the diameter of the wire ( ± 0.005mm or ± 5x10-6m)

Multimeter to measure the resistance ( ± 0.01Ω)

Ruler to measure the length ( ± 1mm or ± 1x10-3m)

Shaded columns require measurements, plain columns require calculations

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Material | Diameter  (mm) | Diameter (m) | Radius (m) | Resistance (Ω) | Length (m) | Coefficient of resistivity (Ωm) |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

Select one wire and try measuring the resistance of your wire at different lengths.

|  |  |
| --- | --- |
| Length (m) | Resistance (Ω) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

How does changing the length of wire affect resistance?

How could the car be designed to reduce electrical resistance?

Taking all the properties into account, which material will make the best electrical connectors and which will make the best wires in a Greenpower car?